DON’T DUMP IT

…unless you know it can go down the drain!

Neutral pH ONLY (measured 5.5 – 12)

Room temperature liquids ONLY (no liquid nitrogen)

No Acetone

No Hazardous Waste

DON’T ASSUME

ALL treated, hazardous waste discharged to the sewer MUST be logged.
[bookmark: _GoBack]Read the Laboratory Safety Manual, Section 3 page 11 for thorough description
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